Installation requirements

Hardware

The hardware requirements directly depends on the number of SAP systems that you want to monitor.​

SAP systems	CPU	Application Memory	Disk
<10	2 Cores	2 GB	30 GB
<30	2 Cores	3 GB	30 GB
<50	4 Cores	4 GB	30 GB
<100	4 Cores	5 GB	60 GB
>100	4 Cores	8 GB	60 GB

​ ​

Software

Supported OS:

Windows server 2012 / 2016

Linux CentOS/SUSE/RedHat

Mandatory software:

Java JRE v1.8 64 bits

SAP JCO drivers for SAP NetWeaver systems

SAP HANA drivers for HANA systems

Network

SAP system type	Ports to open (defaults)
SAP NetWeaver	36XX (Message server) 33XX (App. Server) 5XX13 5XX14 5XX00
SAP HANA	3XX13 3XX15
SAP BusinessObjects	64XX XX: System number

Users and authorizations

NetWeaver - ABAP:

Pro.Monitor uses a Communications data user associated with the provided authorization profile

In most cases, user can be created in client 000. But sometimes access to target client must be necessary as well.

NetWeaver - SAPControl:

Pro.Monitor uses SAPControl web services to collect information on the system.

The access to these services can be controlled by using an OS user and associate it with the appropriate groups and authorizations, as defined in Note 927637

Look for the section describing the use of service/protectedwebmethods, make sure to allow the access of all Getter/Reader services

HANA:

SQL user associated with MONITORING role​

BusinessObjects: ​

User access to CMS repository and CMC portal