Alarms and Metrics

Purpose

Define a general configuration for Alarms and Metrics

Configuration

Two alerts system availability alerts :

Connection problem : Alert generated as soon as a connector check fails

System not responding : Alert generated after several connector check retries

Change the configuration system availability alerts

Define the severity and the Subsystem Id of system availability Alarm.

From the top right of the screen, click on the setting icon

Select the admin configuration sub-menu

Click on tabs Alarms/Metrics

Define the severity

Configuration

Two alerts system availability alerts :

Connection problem : Alert generated as soon as a connector check fails

System not responding : Alert generated after several connector check retries

Change the configuration system availability alerts

Define the severity and the Subsystem Id of system availability Alarm.

From the top right of the screen, click on the setting icon

Select the admin configuration sub-menu

Click on tabs Alarms/Metrics

Define the severity

Internal alerts

Purpose

Internal alert allow the possibility to send alert when Pro.Monitor :

fails to execute a given monitor job

detects a license error

detects a memory issue (low memory)

Change the configuration internal alert

Define the severity of internal alert :

From the top right of the screen, click on the setting icon

Select the admin configuration sub-menu

Click on tabs Alarms/Metrics

Define the severity tend

Configuration

Monitor job execution error : Send an alert if an error occurred when running monitor

CCMS error : Send an alert if an error occurred when running CCMS

License error : Send an alert if a license is expired or not valide

Probe low memory : Send an alert if Pro.Monitor is low memory

Mail gateway

Purpose

Pro.Monitor needs to be configured to enable its send report by email feature.

Configuration

Server : Domain name of IP of SMTP server

Port : port SMTP server * From : Mail sender * User name : User SMTP * Password : Password SMTP ===== LDAP ===== ==== Purpose ==== * Pro.Monitor can use a LDAP for handle the users Pro.Monitor. * The first time connection to Pro.Monitor with LDAP send a request authorization. * The admin must accept the request for allow the access (a notification will be visible) ==== Configuration ==== * URL : URL LDAP server * Example : ldap://nameServer.domainName/dc=DC1,dc=DC2 * Base : Group LDAP * Example : OU=Users,OU=AGL * Filter : * Example : sAMAccountName={0} * Manage DN : User LDAP connection * Manager password :** Password LDAP connection

Change the configuration system availability alerts

Define the severity and the Subsystem Id of system availability Alarm.

From the top right of the screen, click on the setting icon

Select the admin configuration sub-menu

Click on tabs Alarms/Metrics

Define the severity